**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**ARCHITECTURE, ENGINEERING AND CONSTRUCTION**

ARCHITECTURE & ENGINEERING

326 East Hoover, Mail Stop B

Ann Arbor, MI 48109-1002

Phone: 734-764-3414

Fax: 734-936-3334

DOCUMENTS

SPECIFICATION DIVISION 12

NUMBER SECTION DESCRIPTION

DIVISION 12 FURNISHINGS

SECTION 122200 - CURTAINS AND DRAPES

END OF CONTENTS TABLE

1. DIVISION 12 FURNISHINGS
	1. SECTION 122200 - CURTAINS AND DRAPES
		1. GENERAL
			1. SUMMARY
				1. Types of curtains include:

Manually operated, room dividing, lightproof curtains.

Manually operated, lightproof curtains over wall openings.

* + - 1. RELATED WORK OF OTHER SECTIONS
				1. Division 05 Section "Metal Fabrications" for sheet metal valences and trim.
				2. Division 06 Section "Interior Architectural Woodwork" for wood trim.
			2. SUBMITTALS
				1. Product Data: Manufacturer's literature indicating compliance with requirements.
				2. Samples: Submit samples of materials and finishes.
				3. Shop Drawings: Submit shop drawings for installations not fully detailed in product data.
			3. QUALITY ASSURANCE
				1. Provide complete assemblies produced by one mfr for each type required including hardware, accessory items, mounting brackets, and fastenings.
				2. Provide units that are fire retardant treated to comply with NFPA 701 flammability test requirements.
		1. PRODUCTS
			1. CURTAIN FABRIC
				1. Fabric, General: Fire-retardant treated rayon-acetate blend with vinyl backing. For all applications, provide double faced curtains with fabric material on both sides.
				2. Room Dividing Curtains: Provide 2 curtains, both fabricated to cover half the room width plus 1-1/2 feet, resulting in 3-foot total overlap. Fabricate curtains without pleats.

Accessories: Provide Velcro male and female fastening strips for wall ends of curtain units, Apply continuous Velcro fasteners to wall ends of curtain units and on walls as shown, to provide positive, lightproof seal.

* + - * 1. Curtains at Wall Openings: Fabricate curtains to cover opening widths plus 4 feet, resulting in 2-foot overlap at both sides of opening. Fabricate curtains without pleats.

below example describes a lightproof curtain fabric. modify to suit project.

* + - * 1. Manufacturer/Product: Coral Co; "Stoplight II".

Color: "Flax".

* + - 1. TRACKS AND CARRIERS
				1. Provide Manufacturer's standard anodized aluminum or painted steel units without splices.

Provide ball bearinged carrier and hook assemblies.

below example describes a curtain track. modify to suit project.

* + - * 1. Manufacturer/Model: Provide products as follows:

Tracks: Graber; model 9-8191.

* + 1. EXECUTION
			1. INSTALLATION
				1. Examine support work for tracks in presence of Installer. Correct conditions that would result in improper operation of curtain units.
				2. Comply with manufacturer's recommended installation procedures for indicated installation conditions, and as indicated on drawings.

END OF SECTION 122200